* 1. **Knapp Connector T- Joint**

Manufacturing of choose the connection with Knapp connecting systems.

Choose the dimension and the screw joint with select the size of screw . The connection is made in accordance with the manufacturer's instruction manual.

The T-Joint connecting system consists of an angle washer made of cast stainless steel, that is flush mounted in wood or wood-derived materials. The angle washer is available in 20 mm, 30 mm, and 35 mm diameter. The thread angle of the load-bearing screw is 45° or 30°. The 30- and 35-mm diameter connectors are fastened with two KNAPP CS-screws Ø 5 mm or Ø 6 mm. KNAPP CS-screws Ø 6, 8, 10 and 12 mm are available for the load bearing.

Quantity: …………………. Unit Price: ……………………… Total Price: ……………………..

* 1. **Structural connection with the connecting system**

Manufacturing of select the type of connection. The connection is made in accordance with the manufacturer's instruction manual.

Base of planning:

Knapp Connector

Choose a connector size and the screws joint with select the size of screw

The T-Joint connecting system consists of an angle washer made of cast stainless steel, that is flush mounted in wood or wood-derived materials. The angle washer is available in 20 mm, 30 mm, and 35 mm diameter. The thread angle of the load-bearing screw is 45° or 30°. The 30- and 35-mm diameter connectors are fastened with two KNAPP CS-screws Ø 5 mm or Ø 6 mm. KNAPP CS-screws Ø 6, 8, 10 and 12 mm are available for the load bearing.

Or equivalent.

Offered product: ………………………………………………………………………….

Quantity: …………………. Unit Price: ……………………… Total Price: ……………………..